                                                                   Revision : 01
--------------------------------------------------------------------------------
Software name      BIOS Update Utility

Support model      ThinkPad W510

Operating Systems  Microsoft Windows 8  32-bit, 64-bit
                   Microsoft Windows 7  32-bit, 64-bit
                   Microsoft Windows Vista  32-bit, 64-bit
                   Microsoft Windows XP  Professional x64 Edition SP2
                   Microsoft Windows XP  Professional SP3

                   Refer to marketing materials to find out what computer models
                   support which Operating Systems.

Versions           1.45  (for BIOS ID 6Nxxxxxx-based computer)
                   1.45  (for BIOS ID 6Lxxxxxx-based computer)


--------------------------------------------------------------------------------
WHAT THIS PACKAGE DOES

  This package updates two sets of the BIOSes (including system programs and
  Embedded Controller programs) stored in the following ThinkPad computers to
  fix problems, add new functions, or expand functions as noted below.

  - BIOS ID 6Nxxxxxx-based computer
      (Upper two alphanumeric characters of BIOS ID are 6N)
  - BIOS ID 6Lxxxxxx-based computer
      (Upper two alphanumeric characters of BIOS ID are 6L)

  This program is language independent and can be used with any language system.


--------------------------------------------------------------------------------
CHANGES IN THIS RELEASE


Version 1.45  (BIOS ID: 6NET84WW)  [for BIOS ID 6Nxxxxxx-based computer]
------------------------------------------------------------------------

[Important updates]
- Added support for Microsoft Windows 8.

[New functions or enhancements]
- Added support for the function to disable & unconfigure AMT via WMI.
- Updated CompuTrace ROM.

[Problem fixes]
  Nothing.


Version 1.45  (BIOS ID: 6LET84WW)  [for BIOS ID 6Lxxxxxx-based computer]
------------------------------------------------------------------------

[Important updates]
- Added support for Microsoft Windows 8.

[New functions or enhancements]
- Added support for the function to disable & unconfigure AMT via WMI.
- Updated CompuTrace ROM.

[Problem fixes]
  Nothing.


--------------------------------------------------------------------------------
KNOWN LIMITATIONS

- After backing up a Windows XP system to a hard drive connected to the e-SATA
  port through Rescue and Recovery, when attempting to restore the backup image
  from the e-SATA hard drive through Rescue and Recovery, a blue screen error
  occurs. Rescue and Recovery can not access the e-SATA hard drive.


--------------------------------------------------------------------------------
DETERMINING WHICH VERSION IS INSTALLED

  There are two ways to check the BIOS version and BIOS ID.


 [Checking on Windows]

  Windows 8:

  1. Hold down the Windows logo key and press X to open a menu at the lower-left
     area of the screen.

  2. Select Control Panel from the menu.
  3. Make sure "View by Category" is selected, and select System and Security,
     select Administrative Tools, and then select and open System Information.
     - or -
  2. Select Run from the menu.
  3. Type msinfo32, and press Enter.

  4. On the System Information window, make sure System Summary is selected in
     the left side of the window.
  5. Locate the BIOS version/date line in the right side of the window.
     "LENOVO BIOS ID (BIOS version), date" will be shown.

  If you are prompted for an administrator password or confirmation, type your
  password, or click Continue.

  Windows 7/Vista:

  1. Click Start, click All Programs or Programs, click Accessories, click
     System Tools and then click System Information.
     - or -
     Click Start, type msinfo32 in the Start Search box and then click msinfo32
     in the Programs list.
  2. On the System Information window, make sure System Summary is selected in
     the left side of the window.
  3. Locate the BIOS version/date line in the right side of the window.
     "LENOVO BIOS ID (BIOS version), date" will be shown.

  If you are prompted for an administrator password or confirmation, type your
  password, or click Continue.

  Windows XP:

  1. Click Start, click All programs, click Accessories, click System Tools and
     then click System Information.
     - or -
     Click Start, click Run, type msinfo32 in the Open box and then click OK.
  2. On the System Information window, make sure System Summary is selected in
     the left side of the window.
  3. Locate the BIOS version/date line in the right side of the window.
     "LENOVO BIOS ID (BIOS version), date" will be shown.


 [Checking on BIOS Setup]

  Windows 8:
  1. Turn on the computer to start Windows.
  2. Hold down the Windows logo key and press C to open the Charm bar on the
     screen.
  3. Select Settings, then Power from the menu.
  4. Select Reboot to restart the computer.

  Windows 7/Vista/XP:
  1. Turn off the computer.
  2. Turn on the computer.
  3. Go to the step 5.

  5. While the "To interrupt normal startup, press the blue ThinkVantage button"
     message is displayed at the lower-left area of the screen, press the F1 key.
     The BIOS Setup Utility menu will be displayed. If a password prompt appears,
     type the correct password.
  6. Locate the BIOS Version line and Embedded Controller Version line.
     "BIOS version (BIOS ID)" will be shown on the BIOS Version line.
  7. Turn off the computer.


--------------------------------------------------------------------------------
NOTES

- If you use Windows Vista, before applying this BIOS into the system, you
  should install Windows Vista KB 937500. The information of KB937500 is located
  in the following Microsoft's site.
    http://support.microsoft.com/kb/937500/en-us

  To verify if KB937500 is installed properly,
  1. Click Start, then click Control Panel.
  2. Find 'Programs and Features' and click. If this option does not exist on
     the window, choose Classic View to find it.
  3. On 'Tasks' pane, click on "View installed updates".
  4. Verify that KB937500 is included in the list of installed updates.


--------------------------------------------------------------------------------
UPDATING THE BIOS

Notes:
- If your computer runs satisfactorily now, it may not be necessary to update
  the BIOS. To determine if you should update the BIOS, refer to the Version
  Information section.
- You need an AC adapter and a charged battery pack.
- Remove the Power-on password prior to updating the BIOS in the remote
  deployment environments.


Attention:
  Do not turn off or suspend the computer until the update has been completed.
  IF YOU DO THAT WHILE THE UPDATE IS STILL IN PROGRESS, THE SYSTEM BOARD MAY
  HAVE TO BE REPLACED.


Manual Update

  This section assumes to use Internet Explorer and Windows Explorer.

  Downloading file
  1. Click once on the underlined file name. Once this is done, some pop-up
     windows will appear.
  2. Follow the instructions on the screen.
  3. In the window to choose Run or Save, click Save.
  4. Choose the folder you would like to download the file to and click Save.
     A different window will appear and the download will begin and complete.
     Once the download has completed, there may or may not be a message stating
     that the download completed successfully.

  Extracting file
  5. Make sure to be logged on with an administrator account on the target
     computer.
  6. Make sure the AC adapter is firmly connected to the target computer.
  7. Locate the folder where the file was downloaded.
  8. Locate the file that was downloaded and double-click it.
  9. Follow the instructions on the screen.
 10. In the Select Destination Location window, click Next. If you would like to
     select a different folder, click Browse.
 11. In the Ready to Install window, click Install. All the necessary files will
     be extracted to the folder selected in the step 10.

  Updating the BIOS
 12. Make sure the checkbox next to "Install ..... now" is checked and click
     Finish.
 13. Follow the instructions on the screen.
 14. Select 'Update ThinkPad BIOS' and follow the instructions on the screen.
 15. After the update has been completed, the program shows a message 'Flash
     Update has been successfully completed...'. Follow the instructions on the
     screen to restart the computer.

  Finally delete the file saved in the step 4.


Unattended Update

  This is for system administrators' use only.

  1. Refer to the Manual Update section, and download and extract the file.
  2. In the step 12 of the Installing files section, uncheck the checkbox next
     to "Install ..... now", and then click Finish to cancel installation.
  3. At the command line, execute WINUPTP.EXE with the -s option.
     Example: [Path where the files were extracted]\WINUPTP -s

  To view the update result, refer to the WINUPTP.log file created at the same
  directory of the package.


--------------------------------------------------------------------------------
INITIALIZING BIOS

  BIOS Initialization is suggested for some problems. To initialize the BIOS
  settings:

 Windows 8:
  1. Turn on the computer to start Windows.
  2. Hold down the Windows logo key and press C to open the Charm bar on the
     screen.
  3. Select Settings, then Power from the menu.
  4. Select Reboot to restart the computer.

  Windows 7/Vista/XP:
  1. Turn off the computer.
  2. Turn on the computer.
  3. Go to the step 5.

  5. While the "To interrupt normal startup, press the blue ThinkVantage button"
     message is displayed at the lower-left area of the screen, press the F1 key.
     The BIOS Setup Utility menu will be displayed. If a password prompt appears,
     type the correct password.
  6. Press the F9 key to load default configuration.
  7. Select Yes.
  8. Press the F10 key to save default configuration and exit.
  9. Select Yes.
 10. Restart the computer.

  Note:
  After initialization you may need to reapply some settings that you had
  changed previously.


--------------------------------------------------------------------------------
VERSION INFORMATION

  The following versions of BIOSes and ECPs (Embedded Controller Programs) have
  been released to date.


[For BIOS ID 6Nxxxxxx-based computer]
(Upper two alphanumeric characters of BIOS ID are 6N)
-----------------------------------------------------

  Package  (ID)     BIOS  (BIOS ID)   ECP   (ECP ID)      Rev.  Issue Date
  ----------------  ---------------  -----------------    ----  ---------------
  1.45  (6NUJ29US)  1.45  (6NET84WW)  1.21  (6MHT46WW)    01    2012/10/22
  1.44  (6NUJ28US)  1.44  (6NET83WW)  1.21  (6MHT46WW)    01    2012/06/27
  1.43  (6NUJ27US)  1.43  (6NET82WW)  1.21  (6MHT46WW)    01    2012/06/12
  1.42  (6NUJ26US)  1.42  (6NET81WW)  1.21  (6MHT46WW)    01    2012/03/14
  1.41  (6NUJ25US)  1.41  (6NET80WW)  1.21  (6MHT46WW)    01    2011/12/12
  1.40              1.40  (6NET79WW)  1.21  (6MHT46WW)    01    2011/10/21
  1.39              1.39  (6NET78WW)  1.21  (6MHT46WW)    01    2011/08/11
  1.38              1.38  (6NET77WW)  1.20  (6MHT45WW)    01    2011/06/13
  1.37              1.37  (6NET76WW)  1.19  (6MHT44WW)    01    2011/03/23
  1.34              1.34  (6NET74WW)  1.18  (6MHT43WW)    01    2010/11/12
  1.32              1.32  (6NET72WW)  1.15  (6MHT40WW)    01    2010/09/17
  1.27              1.27  (6NET64WW)  1.14  (6MHT39WW)    02    2010/08/12
  1.27              1.27  (6NET64WW)  1.14  (6MHT39WW)    01    2010/08/06
  1.24-1.13         1.24  (6NET61WW)  1.13  (6MHT38WW)    02    2010/06/15
  1.24-1.13         1.24  (6NET61WW)  1.13  (6MHT38WW)    01    2010/06/11
  1.20-1.12         1.20  (6NET57WW)  1.12  (6MHT37WW)    01    2010/06/01
  1.19-1.11         1.19  (6NET56WW)  1.11  (6MHT36WW)    01    2010/05/19
  1.17-1.10         1.17  (6NET54WW)  1.10  (6MHT35WW)    01    2010/04/23
  1.15-1.09         1.15  (6NET52WW)  1.09  (6MHT34WW)    01    2010/03/31
  1.12-1.08         1.12  (6NET49WW)  1.08  (6MHT33WW)    01    2010/03/10
  1.09-1.07         1.09  (6NET46WW)  1.07  (6MHT32WW)    01    2010/02/10
  1.09-1.06         1.09  (6NET46WW)  1.06  (6MHT31WW)          For factory use
  1.08-1.04         1.08  (6NET45WW)  1.04  (6MHT29WW)    02    2010/02/02
  1.08-1.04         1.08  (6NET45WW)  1.04  (6MHT29WW)    01    2010/01/19


[For BIOS ID 6Lxxxxxx-based computer]
(Upper two alphanumeric characters of BIOS ID are 6L)
-----------------------------------------------------

  Package  (ID)     BIOS  (BIOS ID)   ECP   (ECP ID)      Rev.  Issue Date
  ----------------  ---------------  -----------------    ----  ---------------
  1.45  (6NUJ29US)  1.45  (6LET84WW)  1.21  (6MHT46WW)    01    2012/10/22
  1.44  (6NUJ28US)  1.44  (6LET83WW)  1.21  (6MHT46WW)    01    2012/06/27
  1.43  (6NUJ27US)  1.43  (6LET82WW)  1.21  (6MHT46WW)    01    2012/06/12
  1.42  (6NUJ26US)  1.42  (6LET81WW)  1.21  (6MHT46WW)    01    2012/03/14
  1.41  (6NUJ25US)  1.41  (6LET80WW)  1.21  (6MHT46WW)    01    2011/12/12
  1.40              1.40  (6LET79WW)  1.21  (6MHT46WW)    01    2011/10/21
  1.39              1.39  (6LET78WW)  1.21  (6MHT46WW)    01    2011/08/11
  1.38              1.38  (6LET77WW)  1.20  (6MHT45WW)    01    2011/06/13
  1.37              1.37  (6LET76WW)  1.19  (6MHT44WW)    01    2011/03/23
  1.35              1.35  (6LET74WW)  1.18  (6MHT43WW)    01    2010/11/12
  1.33              1.33  (6LET72WW)  1.15  (6MHT40WW)    01    2010/09/17
  1.32              1.32  (6LET67WW)  1.14  (6MHT39WW)    02    2010/08/12
  1.32              1.32  (6LET67WW)  1.14  (6MHT39WW)    01    2010/08/06
  1.31-1.13         1.31  (6LET66WW)  1.13  (6MHT38WW)          For factory use
  1.26-1.13         1.26  (6LET63WW)  1.13  (6MHT38WW)          For factory use


  Note: Revision number (Rev.) is for administrative purpose of this README
        document and is not related to software version. There is no need to
        upgrade this software when the revision number changes.

  To check the version of BIOS and Embedded Controller Program, refer to the
  Determining which version is installed section.


Summary of Changes

  Where: <   >        Package version
         BIOS:        BIOS version
         ECP:         Embedded Controller Program version
         [Important]  Important update
         (New)        New function or enhancement
         (Fix)        Correction to existing function


[For BIOS ID 6Nxxxxxx-based computer]
(Upper two alphanumeric characters of BIOS ID are 6N)
-----------------------------------------------------

<1.45>
 BIOS: 1.45 / ECP: 1.21
- [Important] Added support for Microsoft Windows 8.
- (New) Added support for the function to disable & unconfigure AMT via WMI.
- (New) Updated CompuTrace ROM.

<1.44>
 BIOS: 1.44 / ECP: 1.21
- (New) Added support for the disabling feature of Wireless LAN Controller Link.
- (Fix) Fixed an issue that might shut down the computer by disabling the Intel
        (R) AMT Control option in the BIOS Setup.
        (Note)
        For fix this issue, update Intel AMT 6.2 Management Engine Firmware to
        version 6.2.30.1040 or higher.

<1.43>
 BIOS: 1.43 / ECP: 1.21
- (New) Updated Intel MEBx.

<1.42>
 BIOS: 1.42 / ECP: 1.21
- (Fix) Fixed an issue where the setting of SATA Controller Mode Option in BIOS
        Setup Utility could not be changed through Windows Management
        Instrumentation (WMI) on Windows PE.

<1.41>
 BIOS: 1.41 / ECP: 1.21
- (New) Updated CPU microcode.

<1.40>
 BIOS: 1.40 / ECP: 1.21
- (Fix) Fixed an issue where the bluetooth device disabled when a USB3.0 Hub
        installed.

<1.39>
 BIOS: 1.39 / ECP: 1.21
- (New) Added a message for precaution at handling slice battery.
- (Fix) Fixed an issue where display blackout might occur by uninstalling video
        driver on the system with Windows Vista or Windows 7.

<1.38>
 BIOS: 1.38 / ECP: 1.20
- (New) Support for ME6.2 Host Based Configuration function.
- (New) Support for new video RAM.
- (Fix) Fixed an issue where keyboard on Intel AMT KVM remote console might
        malfunction.

<1.37>
 BIOS: 1.37 / ECP: 1.19
- (Fix) Fixed an issue where the machine might go to shut_down by a certain
        operation during BIOS/H8 flash.
- (Fix) Fixed an issue where the machine might go to shut_down by removing the
        slice battery(FRU#42T4739) during suspend mode.

<1.34>
 BIOS: 1.34 / ECP: 1.18
- (New) Added support of "Power On with AC Attach" feature at BIOS Setup Utility
        -> Config -> Power submenu.
- (Fix) Fix an issue that a USB device is not recognized by Windows connecting
        to USB 3.0 port.

<1.32>
 BIOS: 1.32 / ECP: 1.15
- (New) Added support for new CPU models.

<1.27>
 BIOS: 1.27 / ECP: 1.14
- (Fix) Corrected an description of VERSION INFORMATION in this README document.
        (BIOS ID 6Nxxxxxx-based computer's version number.)

<1.27>
 BIOS: 1.27 / ECP: 1.14
- (Fix) Fixed an issue where the setting of SATA Controller Mode Option in BIOS
        Setup Utility could not be changed through Windows Management
        Instrumentation (WMI).
- (Fix) Fixed an issue where the computer might not be powered on by pressing
        the power button of the Docking Station while the LCD was closed.
- (Fix) Fixed an issue where the computer might not resume normal operation from
        suspend/standby/sleep state when a hard disk password was installed and
        Intel TXT Feature in BIOS Setup Utility was enabled.

<1.24-1.13>
 BIOS: 1.24 / ECP: 1.13
- (Fix) Added an description of Windows XP x64 in Operating Systems in this
        README document.

<1.24-1.13>
 BIOS: 1.24 / ECP: 1.13
- (New) Enable OS boot support from e-SATA strage device.
        (Harddisk Password in external harddisk is not supported.)
- (Fix) Fix an issue where an invalid password error is encountered when
        attempting to use a supervisor password as a current password while an
        user logons BIOS setup with a supervisor password.
- (Fix) Fix an issue where usable memory is displayed under 3GB on 64bit OS even
        4GB or more memory installed.
- (Fix) Fix an issue that a USB device is not recognized by Windows connecting
        to the Alway On USB enabled port.

<1.20-1.12>
 BIOS: 1.20 / ECP: 1.12
- (New) Adding disabling option for unsupported AC adapter warning message.
- (Fix) Fixed an issue where showing incorrect power consumption with docking
        station.

<1.19-1.11>
 BIOS: 1.19 / ECP: 1.11
- (Fix) Fixed an issue where screen garbage might be displayed with 2nd HDD in
        Ultrabay during resuming from suspend.
- (Fix) Fixed an issue where a incorrect IP address of HPM (Hardware Password
        Manager) server might be displayed on HPM logon screen.

<1.17-1.10>
 BIOS: 1.17 / ECP: 1.10
- (Fix) Fixed an issue where the screen might not be displayed on LCD panel on
        NVIDIA NVS 3100M model when system booted with closed LCD.
- (Fix) Fixed an issue where system might not be resumed on non-Windows ACPI OS.

<1.15-1.09>
 BIOS: 1.15 / ECP: 1.09
- [Important]
        Prevents from preload 64-bit Windows re-activation after updating a BIOS.
        (This BIOS fix does not resolve re-activation request itself)
        (This problem does not affect when BIOS updating by BIOS Update CD)
- (New) Improve key input response.
- (Fix) Fixed an issue where StartUp Interrupt Menu can not be displayed by
        condition.
- (Fix) For vPro users: Fixed an issue where multiple provisioning data handling
        by USB key provisioning does not work.
- (Fix) Fixed an issue where network boot may not be executed via ethernet
        device.
- (Fix) Fixed an issue where system might not boot with  USB PortReplicator
        attached to USB3.0 port.
- (Fix) Fixed an issue where screen may not displayed on LCD panel when pressing
        Fn+F7 key when system boot with closed LCD.
- (Fix) Fixed an issue optical media may not be ejected by once pressing eject
        button.

<1.12-1.08>
 BIOS: 1.12 / ECP: 1.08
- (Fix) Corrected an description of Version of CHANGES IN THIS RELEASE in this
        README document.

<1.12-1.08>
 BIOS: 1.12 / ECP: 1.08
- (New) Improved the waiting time indication for security chip related
        operations.
- (New) Optimized the waiting time for security chip operations as per device.
- (New) Optimized graphics device settings.
- (New) Updated Lenovo and Phoenix copyright year to 2010.
- (Fix) Fixed an issue where block-noise appeared on the screen when playing the
        video through the IEEE 1394 port.
- (Fix) Fixed an issue where the ExpressCard device might not work after
        restarting the computer.
- (Fix) Fixed an issue that Disabling Intel AMT option in the BIOS Setup menu
        did not function correctly.
- (Fix) Fixed an issue where system might be shutdown instead of restarting when
        embedded controller program was updated.

<1.09-1.07>
 BIOS: 1.09 / ECP: 1.07
- [Important]
        Added support for Microsoft Windows XP Professional x64 Edition SP2.
- (Fix) Fixed an issue where battery authentication might be failed.

<1.09-1.06>
 BIOS: 1.09 / ECP: 1.06
- (New) Adjusted LED brightness of mic mute button.
- (Fix) Fixed an issue where main battery would be used first even though main
        and sub battery are attached.
- (Fix) Fixed an issue where battery charging was stopped if the battery's
        current capacity was over than "Start charging" capacity at resuming
        from sleep state.

<1.08-1.04>
 BIOS: 1.08 / ECP: 1.04
- (Fix) Corrected an description of Operating Systems and Version in this README
        document.

<1.08-1.04>
 BIOS: 1.08 / ECP: 1.04
- (New) Initial release for ThinkPad W510.


[For BIOS ID 6Lxxxxxx-based computer]
(Upper two alphanumeric characters of BIOS ID are 6L)
-----------------------------------------------------

<1.45>
 BIOS: 1.45 / ECP: 1.21
- [Important] Added support for Microsoft Windows 8.
- (New) Added support for the function to disable & unconfigure AMT via WMI.
- (New) Updated CompuTrace ROM.

<1.44>
 BIOS: 1.44 / ECP: 1.21
- (New) Added support for the disabling feature of Wireless LAN Controller Link.
- (Fix) Fixed an issue that might shut down the computer by disabling the Intel
        (R) AMT Control option in the BIOS Setup.
        (Note)
        For fix this issue, update Intel AMT 6.2 Management Engine Firmware to
        version 6.2.30.1040 or higher.

<1.43>
 BIOS: 1.43 / ECP: 1.21
- (New) Updated Intel MEBx.

<1.42>
 BIOS: 1.42 / ECP: 1.21
- (Fix) Fixed an issue where the setting of SATA Controller Mode Option in BIOS
        Setup Utility could not be changed through Windows Management
        Instrumentation (WMI) on Windows PE.

<1.41>
 BIOS: 1.41 / ECP: 1.21
- (New) Updated CPU microcode.

<1.40>
 BIOS: 1.40 / ECP: 1.21
- (Fix) Fixed an issue where the bluetooth device disabled when a USB3.0 Hub
        installed.

<1.39>
 BIOS: 1.39 / ECP: 1.21
- (New) Added a message for precaution at handling slice battery.
- (Fix) Fixed an issue where display blackout might occur by uninstalling video
        driver on the system with Windows Vista or Windows 7.

<1.38>
 BIOS: 1.38 / ECP: 1.20
- (New) Support for ME6.2 Host Based Configuration function.
- (New) Support for new video RAM.
- (Fix) Fixed an issue where keyboard on Intel AMT KVM remote console might
        malfunction.

<1.37>
 BIOS: 1.37 / ECP: 1.19
- (Fix) Fixed an issue where the machine might go to shut_down by a certain
        operation during BIOS/H8 flash.
- (Fix) Fixed an issue where the machine might go to shut_down by removing the
        slice battery(FRU#42T4739) during suspend mode.

<1.35>
 BIOS: 1.35 / ECP: 1.18
- (New) Added support of "Power On with AC Attach" feature at BIOS Setup Utility
        -> Config -> Power submenu.
- (Fix) Fix an issue that a USB device is not recognized by Windows connecting
        to USB 3.0 port.

<1.33>
 BIOS: 1.33 / ECP: 1.15
- (New) Added support for new CPU models.

<1.32>
 BIOS: 1.32 / ECP: 1.14
- (Fix) Corrected an description of VERSION INFORMATION in this README document.
        (BIOS ID 6Nxxxxxx-based computer's version number.)

<1.32>
 BIOS: 1.32 / ECP: 1.14
- (Fix) Fixed an issue where the setting of SATA Controller Mode Option in BIOS
        Setup Utility could not be changed through Windows Management
        Instrumentation (WMI).
- (Fix) Fixed an issue where the computer might not be powered on by pressing
        the power button of the Docking Station while the LCD was closed.
- (Fix) Fixed an issue where the computer might not resume normal operation from
        suspend/standby/sleep state when a hard disk password was installed and
        Intel TXT Feature in BIOS Setup Utility was enabled.

<1.31-1.13>
 BIOS: 1.31 / ECP: 1.13
- (Fix) Fixed some issues during the production process.

<1.26-1.13>
 BIOS: 1.26 / ECP: 1.13
- (New) Initial release for ThinkPad W510 new model.


--------------------------------------------------------------------------------
BIOS INFORMATION

Memory Map Information
----------------------


Reserved Area:
The following conventional memory addresses are reserved by the BIOS and others.

 NVIDIA Quadro FX 880M model

  C0000-CFBFF : Reserved for Video BIOS
  D0000-D1FFF : Reserved for Option ROM of Ethernet (*a)
  D2000-D87FF : Reserved for Option ROM of RAID
  DD000-DFFFF : Reserved for USB BIOS (*b)
  E0000-FFFFF : Reserved for System BIOS

   *a: This area becomes free by disabling the Ethernet LAN Option ROM option
       under Config and Network in the BIOS Setup Utility. This choice will
       disable PXE and WOL features.
   *b: This area becomes free by disabling the USB BIOS Option ROM option under
       Config and USB in the BIOS Setup Utility. This choice will disable
       booting from USB device and other USB BIOS features.


Usable Area:
The following memory address can be used by the memory manager such as EMM386.

 NVIDIA Quadro FX 880M model

  D8800-DCFFF

  Note:
  Certain addresses in this area will be reserved for optional devices by
  Operating Systems. The addresses vary and depend on the design of each
  Operating System.


--------------------------------------------------------------------------------
LIMITATIONS

  Nothing.


--------------------------------------------------------------------------------
TRADEMARKS

* Lenovo, Rescue and Recovery, ThinkPad and ThinkVantage are registered
  trademarks of Lenovo.

* Absolute and Computrace are registered trademarks of Absolute Software
  Corporation.
* ExpressCard is a trademark of PCMCIA (Personal Computer Memory Card
  International Association).
* NVIDIA is a registered trademark of NVIDIA Corporation.
* Intel is a registered trademark of Intel Corporation.
* Intel vPro is a trademark of Intel Corporation.
* Microsoft, Windows and Windows Vista are registered trademarks of Microsoft
  Corporation.
* Phoenix is a registered trademark of Phoenix Technologies Ltd.
* Phoenix Technologies is a trademark of Phoenix Technologies Ltd.

Other company, product, and service names may be registered trademarks,
trademarks or service marks of others.
