-Manufacturer: Lenovo
-Model : ThinkPad W510 
-Bios Revision: 1.45
-Bios link: http://download.lenovo.com/ibmdl/pub/pc/pccbbs/mobiles/6nuj29us.exe
-Bios Type: Phoenix BIOS

-SLIC: 
-Tools: Phoenix Mod Tool v2.02
-Method: Dynamic+NoSlic + HEX mod for whitelist check "removal"


  This package updates two sets of the BIOSes for ThinkPad W510 system.

  - v.1.45 BIOS ID 6Nxxxxxx-based computer
      (Upper two alphanumeric characters of BIOS ID are 6N)
  - v.1.45 BIOS ID 6Lxxxxxx-based computer
      (Upper two alphanumeric characters of BIOS ID are 6L)

------------

How to flash the bios:

1. FLASH ORIGINAL (non modified) bios - run 6nuj29us.exe as "Administartor"

2. Check BIOS ID with Slictoolkit or other software.

3. Flash modified bios:
  
   - for BIOS ID 6Nxxxxxx-based computer use 6NET84WW folder.

   - for BIOS ID 6Lxxxxxx-based computer use 6LET84WW folder.


for modified bios flashing :

run the WinPhlash (32 or 64 bit), click "Advanced Settings" then check and uncheck the boxes so it looks like this:

("Flags" Tab):
[ ] Verify BIOS part number
[ ] Flash only if BIOS version is different
[ ] Flash only if BIOS version is newer
[ ] Verify BIOS image size
[ ] Verify BIOS checksum
[ ] Zero block before erasing
[x] Verify block after programming
[x] Disable Axx swaping automatic detection (if present)
[ ] Clear CMOS Checksum

("DMI" tab)
"Update": Select "Update the BIOS and not DMI" 


